**SCBA Ensemble Donning**

**Standard:**

NFPA 1001: 4.3.1 2019 Edition

**Task/Performance Outcome:**

The candidate shall demonstrate the ability to safely and correctly donn their full SCBA ensemble within 60 seconds. Upon the candidate clapping their hands, the SCBA should be completely donned and operationally ready according to manufacturer and district guidelines.

**Required Personal Protective Equipment (PPE):**

Full turnout ensemble

**Critical Fail Criteria:**

Failure consists of the following:

* Failure to wear the required PPE
* Failure to physically address their accountability on the passport of their assigned apparatus
* Glaring, gross errors, as documented by the evaluator
* An apparent lack of efficiency and comfort with the activity, as documented by the evaluator
* Less than 80% of available points scored
* A time greater than 60 seconds

**Evolution Details:**

Candidate is kneeling behind their SCBA in their full turnout ensemble. The SCBA is laying in front of the candidate as follows:

* Top of the SCBA towards the candidate
* SCBA harness face up
* SCBA straps are spread out into a circular pattern on each side of the SCBA
* SCBA straps are fully extended
* SCBA is completely turned off
* SCBA face piece standing upright on the nose cup with the face piece netting towards candidate

**SCBA Ensemble Donning**

|  |  |  |
| --- | --- | --- |
| **Actions** | **Points Available** | **Points Earned** |
| **Time starts upon instructor prompt** |  |  |
| Gloves removed | 1 |  |
| SCBA valve opened | 1 |  |
| SCBA pressure stated out loud | 1 |  |
| SCBA vibralert activation stated out loud | 1 |  |
| SCBA PASS activation stated out loud | 1 |  |
| SCBA donned | 1 |  |
| Shoulder straps tightened | 1 |  |
| Waist straps tightened | 1 |  |
| Helmet removed (after SCBA donned for safety) | 1 |  |
| SCBA face piece donned | 1 |  |
| SCBA face piece seal check one stated out loud | 1 |  |
| Nomex hood donned and aligned correctly | 1 |  |
| Helmet is donned and secured with chinstrap and rear fastener | 1 |  |
| SCBA face piece seal check two stated out loud | 1 |  |
| Firefighter gloves donned | 1 |  |
| SCBA regulator donned, breath taken, and no leaks are noted | 1 |  |
| **Time stops upon candidate clapping** | 3 |  |
| **Total (16/19 to pass)** | 19 |  |

0:40 or less = 3 points

0:41 – 0:50 = 2 points

0:51 – 0:60 = 1 point

0:61 or more = Fail

Candidate: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Evaluator: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Total: \_\_\_\_\_\_\_\_/19

Circle one:

Pass/Fail on points/Fail on critical criteria

Comments: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_